#
ON-BOARD DIAGNOSTIC SYSTEM ACTIVE COMMAND MODES FUNCTION (DYNAMIC STABILITY CONTROL)

BHE040243000T04

• The active command modes function is used for optionally selecting active command modes items of input/output parts preset in the DSC HU/CM, and to operate them regardless of CM control.

• To protect the hydraulic unit interior, operate output related parts for only 10 s or less when using the active command modes function.

## Active Command Modes Table

Command name | Output part name | Operation | Operation condition
--- | --- | --- | ---
LATACCEL | Combined sensor (lateral acceleration) initialization start-up | TRUE/FALSE | Ignition switch at ON
LF_DSC_V | LF stability control valve | On/Off
LF_INLET | LF inlet solenoid valve
LF_OUTLET | LF outlet solenoid valve
LF_TC_VLV | LF traction control valve
LR_INLET | LR inlet solenoid valve
LR_OUTLET | LR outlet solenoid valve
PMP_MOTOR | Pump motor
RF_DSC_V | RF stability control valve
RF_INLET | RF inlet solenoid valve
RF_OUTLET | RF outlet solenoid valve
RF_TC_VLV | RF traction control valve
RR_INLET | RR inlet solenoid valve
RR_OUTLET | RR outlet solenoid valve
SAS_CAL | Steering angle sensor initialization start-up | TRUE/FALSE
YAWRATE | Combined sensor (yaw rate) initialization start-up | On/Off