#
AIR BLEEDING

BHE041101021W01

  Caution

  • Brake fluid will damage painted surfaces. Be careful not to spill any on painted surfaces. If it is spilled, wipe it off immediately.

  Note

  • Keep the fluid level in the reserve tank at 3/4 full or more during the air bleeding.
  • Begin air bleeding with the master cylinder and then continue with the brake caliper that is furthest away from the master cylinder. Finish by bleeding air from the master cylinder again.

  Specified fluid

  European (L.H.D. U.K.) specs. | SAE J1703, FMVSS 116 DOT3 or DOT4
  Australian specs. | SAE J1703, FMVSS 116 DOT3

1. Remove the bleeder cap from the brake caliper, and connect a vinyl tube to the bleeder screw.

2. Place the other end of the vinyl tube in a clear container, and fill the container with fluid during air bleeding.

3. Working with two people, one should depress the brake pedal a few times and then depress and hold the pedal down.

4. While the brake pedal is being held down, the other person should loosen the bleeder screw using the SST, and bleed any fluid containing air bubbles. Once completed, tighten the bleeder screw.

  Tightening torque
  6.9-9.8 N·m {71-99 kgf·cm, 62-86 in·lbf}

5. Repeat Steps 3 and 4 until no air bubbles are seen.

6. Perform air bleeding as described in the above procedures for all brake calipers.

7. After air bleeding, inspect the following:

  • Brake operation
  • Fluid leakage
  • Fluid level