#
HOUSING ASSEMBLY III

BHE011002000E10

1. Assemble in the order indicated in the table.

1 | Oil strainer
2 | Oil-level sensor
3 | Oil baffle plate
4 | Clip
5 | Oil pan (See Oil Pan Assembly Note.)
6 | Thermostat component
7 | Water pump body
8 | Engine hanger (engine front side)
9 | Engine coolant temperature sensor
10 | Engine hanger (engine rear side)
11 | Oil filter component

## Oil Pan Assembly Note

  Caution

  • Using bolts with the oil sealant still adhering could cause cracks in the housing. Clean all sealant off all oil pan bolts before assembly.
  • Apply the silicon sealant in a single, unbroken line around the whole perimeter.
  • Install the engine front cover within 5 min after applying the silicone sealant.

1. Completely clean and remove any oil, dirt, sealant or other foreign material that may be adhering to the housing and oil pan.

2. When reusing oil pan installation bolts, clean any old sealant from the bolts.

3. Apply silicone sealant to the areas shown in the figure.

  Bead thickness
  2.5-6.5 mm {0.1-0.2 in}

4. Tighten the oil pan installation bolts.

  Tightening torque
  8.8-11.8 N·m
  {90-120 kgf·cm, 78-104 in·lbf}