#
POWER DOOR LOCK SYSTEM OUTLINE

BHE091401090T01

• Unlocking/locking of all doors is performed by operation of the door key cylinder.

• A double-locking function has been adopted. (When the locking operation using the door key cylinder is performed twice within 3 s, unlocking the door with the door lock knob is inhibited.)

• A lock cancel function has been adopted (When any door is open, locking operation using the door key cylinder or the door lock knob is cancelled and the doors are unlocked.)