#
FRONT PILLAR REMOVAL

BHE098074090B01

1. Rough cut area (A), drill the 42 weld locations indicated by (B), then remove the lower part of the front pillar outer.

  Caution

  • Avoid cutting with a blowtorch or similar tools as the insulator (shaded area) is flammable.

2. Rough cut area (C), drill the 55 weld locations indicated by (D) and one location (E), then remove the front pillar outer and reinforcement.

  Note

  • For weld location (E), partially bend back the cowl upper plate before drilling.

3. Rough cut area (F), drill the 11 weld locations indicated by (G), then remove the front pillar inner.