#
SELECTOR LEVER COMPONENT INSPECTION

BHE051446102W02

1. Remove the engine cover.

2. Remove the battery cover.

3. Disconnect the negative battery cable.

4. Remove the ashtray. (See CONSOLE REMOVAL/INSTALLATION.)

5. Remove the shift knob. (See SELECTOR LEVER REMOVAL/INSTALLATION.)

6. Remove the console panel and indicator assembly. (See SELECTOR LEVER REMOVAL/INSTALLATION.)

7. Disconnect the selector lever component connector.

8. Verify continuity as indicated in the table.

  • If there is any malfunction, replace the selector lever. (See SELECTOR LEVER REMOVAL/INSTALLATION.)