#
WINDSHIELD WIPER AND WASHER SWITCH REMOVAL/INSTALLATION

BHE091966122W03

1. Disconnect the negative battery cable.

2. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Remove the ignition key illumination. (See IGNITION KEY ILLUMINATION BULB REMOVAL/INSTALLATION.)

4. Disconnect the windshield wiper and washer switch connector.

5. Remove the screws, then remove the windshield wiper and washer switch.

6. Install in the reverse order of removal.