#
WINDSHIELD WASHER TANK REMOVAL/INSTALLATION

BHE091967480W01

1. Disconnect the negative battery cable.

2. Disconnect the windshield washer motor connector.

3. Disconnect the headlight cleaner motor connector. (Vehicles with the headlight cleaner)

4. Disconnect the headlight cleaner relay connector. (Vehicles with the headlight cleaner)

5. Disconnect the windshield washer hose from joint pipe A.

6. Disconnect the headlight cleaner hose from joint pipe B. (Vehicles with the headlight cleaner)

7. Remove the bolts, then remove the windshield washer tank.

8. Install in the reverse order of removal.