#
LUMBAR SUPPORT MOTOR INSPECTION

BHE091388664W01

1. Disconnect the lumbar support motor connector.

2. Connect battery positive voltage to lumbar support motor terminal A or B, then verify that the lumbar support motor operate as shown in the table.

  • If the lumbar support motor do not operate as indicated in the table, replace the lumbar support motor.

Motor operation | Connection
--- | ---
B+ | GND
Forward | A (B) | B (A)
Backward | B (A) | A (B)

  ( ) :
R.H.D.