#
INFORMATION DISPLAY REMOVAL/INSTALLATION

BHE092255000W01

1. Disconnect the negative battery cable.

2. Remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

3. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

4. Remove the center panel module. (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)

5. Remove the LCD unit. (See LCD UNIT REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

1 | Screw
2 | Information display

7. Install in the reverse order of removal.