#
FAN MOTOR REMOVAL/INSTALLATION

BHE011215140W01

1. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION.)

4. Drain the engine coolant. (See ENGINE COOLANT REPLACEMENT.)

5. Remove the following.

  (1) Splash shield
  (2) Under cover
  (3) Battery and battery box (See BATTERY REMOVAL/INSTALLATION.)
  (4) Air cleaner component and air cleaner insulator (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)
  (5) PCM duct

6. Position the coolant reserve tank out of the way. (See COOLANT RESERVE TANK REMOVAL/INSTALLATION.)

7. Disconnect the ATF oil cooler hose. (AT)

8. Remove the radiator and cooling fan component. (See RADIATOR REMOVAL/INSTALLATION.)

9. Remove in the order indicated in the table.

1 | Cooling fan No.1
2 | Cooling fan No.2
3 | Cooling fan motor No.1
4 | Cooling fan motor No.2
5 | Radiator cowling

10. Install in the reverse order of removal.

11. Add engine coolant. (See ENGINE COOLANT REPLACEMENT.)

12. Inspect for engine coolant leakage. (See ENGINE COOLANT LEAKAGE INSPECTION.)