#
INTERLOCK CABLE INSPECTION

BHE051409000W02

1. Turn the ignition switch to the ACC or ON position.

2. Verify that the interlock cable moves freely with the brake pedal depressed.

  • If there is any malfunction, replace the interlock cable.
  • If there is any malfunction in the shift lock and the key interlock, but there are no malfunctions in the interlock cable, adjust the interlock cable.

3. After inspection, adjust the interlock cable.

(SeeINTERLOCK CABLE ADJUSTMENT.)