#
FRONT DOOR REMOVAL/INSTALLATION

BHE091158010W02

1. Disconnect the negative battery cable.

2. To remove the checker, remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)
  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)
  (3) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

3. To remove the front door hinge, remove the following parts:

  (1) Front bumper (See FRONT BUMPER REMOVAL/INSTALLATION.)
  (2) Front fender panel (See FRONT FENDER PANEL REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Connector (See Connector Removal Note.)
2 | Bolt A
3 | Bolt B
4 | Front door
5 | Nut
6 | Checker
7 | Bolt C
8 | Front door hinge

5. Install in the reverse order of removal.

6. Adjust the front door. (See DOOR ADJUSTMENT.)

## Connector Removal Note

1. Pull the rubber boot outward.

2. Pull down the lever in the direction indicated by the arrow and disconnect the connector.