#
ON-BOARD DIAGNOSTIC SYSTEM EXTERNAL TESTER COMMUNICATION FUNCTION (DYNAMIC STABILITY CONTROL)

BHE040243000T05

• The external tester communication function enables communication of diagnostic data (DTC read-outs, input/output signal read-outs, and operation of input/output parts) between the DSC HU/CM and an external tester.

## Connections and Communication Contents

| External tester
--- | ---
WDS or equivalent
Connection | Communication method
Self-diagnosis (malfunction detection) function | Input/output: KLN terminal | Serial communication
Data monitor function | Input/output: KLN terminal | Serial communication
Active command modes function | Input/output: KLN terminal | Serial communication

## Serial communication

• Serial communication (two-way communication) allows for multiple data to be sent and received instantly along the same line.

• By connecting the WDS or equivalent to the DLC-2, diagnostic data can be sent and received between the WDS or equivalent and the DSC HU/CM using the KLN terminal (within the DLC-2).

• The DSC HU/CM receives the command signals of the malfunction detection function, PID/data monitor function, and the active command modes function from the WDS or equivalent, and sends DTCs and data regarding the operating condition and status of each input/output part to the WDS or equivalent.

Diagnostic function name | Signal received | Signal sent
--- | --- | ---
Malfunction detection function | DTC verification signal | DTC
PID/data monitor function | Command signal to read selected monitor item | Monitored data for requested monitor item
Active command modes function | Operation command signal for selected active command modes item | Input/output part name