#
ON-BOARD DIAGNOSTIC SYSTEM ACTIVE COMMAND MODES FUNCTION (ELECTRIC POWER STEERING)

BHE060201038T04

• The EPS system can be set to the neutral position using the active command modes function.

Active command modes

Command name (WDS or equivalent) | Output part name | Operation | Operation condition
--- | --- | --- | ---
TRQ_S_CAL | EPS system neutral position setting | ON/OFF | Ignition switch at ON