#
STARTER INSPECTION

BHE011918400W03

## On-vehicle Inspection

1. Verify that the battery is fully charged.

2. The starter is normal if it rotates smoothly and without any noise when the engine is cranked.

  • If the starter does not operate, inspect the following:

  – Remove the starter, and inspect the starter unit.
  – Inspect the related wiring harnesses, the ignition switch, and the transmission range switch (AT).

## No-load test

1. Verify that the battery is fully charged.

2. Connect the starter, battery, and a tester as shown in the figure.

3. Operate the starter and verify that it rotates smoothly.

  • If the starter does not rotate smoothly, inspect the starter unit.

4. Measure the voltage and current while the starter is operating.

  • If not within the specification, replace the starter.

Standard current

Item
Voltage (V) | Current (A)
--- | ---
11 | MT: 90 or less AT: 105 or less