#
ACCESSORY SOCKET REMOVAL/INSTALLATION

BHE092066290W01

1. Disconnect the negative battery cable.

2. Remove the hole cover. (See CONSOLE REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Accessory socket (See Accessory Socket Removal Note.)
2 | Cap (See Cap Removal Note.)

4. Install in the reverse order of removal.

## Accessory Socket Removal Note

1. While pressing a tape-wrapped flathead screwdriver against the cap projection, pull the accessory socket outward.

## Cap Removal Note

1. While pressing the tabs, pull the cap outwards.