#
ON-BOARD DIAGNOSTIC SYSTEM OUTLINE (DYNAMIC STABILITY CONTROL)

BHE040243000T01

• The on-board diagnostic system consists of a malfunction detection system that detects abnormalities in input/output signals when the ignition switch is at the ON position, a data monitor function that reads out specified input/output signals and a simulation function that allows for override operation of output parts (such as solenoid valves).

• The data link connector 2 (DLC-2), which groups together all the connectors used for malfunction diagnosis and detecting/repair into a single location, has been adopted, thereby improving serviceability. Diagnosis is performed by connecting the WDS or equivalent to the DLC-2.

• In addition to DTC read-out, the WDS or equivalent is used to clear DTCs using the display screen of the diagnostic tester, and to access the PID/data monitor and simulation functions, providing enhanced malfunction diagnosis and improved serviceability.

## Block Diagram

1 | DSC indicator light
2 | DSC OFF light
3 | ABS warning light
4 | Brake system warning light
5 | Malfunction indication function
6 | On-board diagnosis function
7 | Serial communication
8 | Memory function
9 | Malfunction detection function
10 | PID/data monitor function
11 | Active command modes function
12 | Fail-safe function
13 | Hydraulic unit inspection function
14 | Input devices
15 | Normal control area
16 | Output devices
17 | WDS or equivalent