#
RADIATOR REMOVAL/INSTALLATION

BHE011215200W01

  Warning

  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.

1. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION.)

4. Drain the engine coolant. (See ENGINE COOLANT REPLACEMENT.)

5. Remove the following.

  (1) Splash shield
  (2) Under cover
  (3) Battery, battery box (See BATTERY REMOVAL/INSTALLATION.)
  (4) Air cleaner component, air cleaner insulator (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)
  (5) PCM duct

6. Position the coolant reserve tank out of the way. (See COOLANT RESERVE TANK REMOVAL/INSTALLATION.)

7. Disconnect the ATF oil cooler hose. (AT)

8. Remove in the order indicated in the table.

9. Install in the reverse order of removal.

10. Add engine coolant. (See ENGINE COOLANT REPLACEMENT.)

11. Inspect for engine coolant leakage. (See ENGINE COOLANT LEAKAGE INSPECTION.)

1 | Connector
2 | Upper radiator hose
3 | Lower radiator hose
4 | Condenser installation bolts
5 | Bracket
6 | Radiator bracket
7 | Radiator
8 | Cooling fan component