#
DRIVE PLATE REMOVAL/INSTALLATION

BHE051319020W01

1. Remove the transmission (See AUTOMATIC TRANSMISSION REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Bolt
2 | Backing plate
3 | Drive plate (See Drive Plate Removal Note.) (See Drive Plate Installation Note.)
4 | Adapter

## Drive Plate Removal Note

1. Set the SST against the engine.

2. Remove the bolts and the drive plate.

## Drive Plate Installation Note

1. Set the SST against the engine.

2. Tighten the drive plate mounting bolts in two or three steps in the order as shown in the figure.

  Tightening torque
  41.2-61.8 N·m
  {4.2-6.3 kgf·m, 30.4-45.5 ft·lbf}

3. Install the transmission. (See AUTOMATIC TRANSMISSION REMOVAL/INSTALLATION.)