#
REAR FENDER RAIN RAIL AND CORNER PLATE INSTALLATION

BHE098070440B02

1. When installing new parts, position each part so that the section measurement aligns with the body dimension

2. Drill holes for plug welds before installing new parts.

3. After temporarily installing new parts, make sure the related parts fit properly.

  Note

  • When replacing the rear fender rain rail and the corner plate separately, weld three locations indicated by (A).