#
ABS CONTROL OPERATION

BHE041543750T11

• When the DSC CM determines wheel slip conditions based on the signals from the ABS wheel-speed sensors during braking, the DSC CM operates the DSC HU inlet and outlet solenoid valves, reducing and maintaining brake fluid pressure in accordance with the wheel slip factors. Then, when the wheel slip condition has passed, brake fluid pressure is increased and maintained, ensuring braking with a constantly stable brake force.

## Operating Condition Transition Diagram

1 | Speed
2 | Solenoid valve control
3 | Pressure reduction
4 | Pressure maintained
5 | Pressure increase
6 | Brake fluid pressure
7 | High
8 | Wheel speed
9 | Estimated vehicle speed
10 | Time