#
WINDSHIELD WIPER MOTOR REMOVAL/INSTALLATION

BHE091967340W01

1. Disconnect the negative battery cable.

2. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

3. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

4. Disconnect the connector.

5. Remove the bolts. Move the windshield wiper motor in the direction of the arrow, remove the securing dowel from the bracket, then remove the windshield wiper motor.

6. Install in the reverse order of removal.