#
WHEEL HUB, STEERING KNUCKLE REMOVAL/INSTALLATION

BHE031104060W02

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the wiring harness if it is pulled by mistake. Before performing the following procedures, disconnect the ABS wheel-speed sensor harness connector (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while servicing the vehicle.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, inspect the front wheel alignment. (See FRONT WHEEL ALIGNMENT.)

1 | ABS wheel-speed sensor connector
2 | Brake caliper component (See Brake Caliper Component Removal Note.)
3 | Mounting support
4 | Disc plate
5 | Tie-rod end (See Tie-rod End Removal Note.)
6 | Stabilizer control link (lower)
7 | Front upper arm ball joint (See Front Upper Arm Ball Joint Removal Note.)
8 | Front upper arm bolt
9 | Front lower arm ball joint (See Front Lower Arm Ball Joint Removal Note.)
10 | Wheel hub, steering knuckle component
11 | Steering knuckle
12 | Dust cover
13 | Wheel hub bolt
14 | Wheel hub component

## Brake Caliper Component Removal Note

1. Remove the brake caliper component installation bolt, and suspend the brake caliper component with a cable in place out of the way.