#
CLOCK SPRING ADJUSTMENT

BHE081066123W02

  Note

  • The adjustment procedure is also specified on the caution label of the clock spring.

1. Set the front tires straight-ahead.

  Caution

  • The clock spring will break if over-wound. Do not forcibly turn the clock spring.

2. Turn the clock spring clockwise until it stops.

3. From the stopped position, turn the clock spring counterclockwise 2 3/4 turns..

4. Align the marks.