#
FRONT COMBINATION LIGHT REMOVAL/INSTALLATION

BHE091851060W01

  Warning

  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the discharge headlight service warnings. (See DISCHARGE HEADLIGHT SERVICE WARNINGS.)

1. Disconnect the negative battery cable.

2. Remove the front side turn lights. (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Bolt A
2 | Bolt B
3 | Bolt C
4 | Cover
5 | Fastener
6 | Connector
7 | Front combination light

5. Install in the reverse order of removal.

6. Adjust the headlight aiming. (SeeHEADLIGHT AIMING)