#
DTC 06:ER07

BHE090266900W19

DTC 06:Er07 | CD changer (upper module)
DETECTION CONDITION | Note • When error occurs, error message "CHECK CD" is displayed in the LCD. • Base unit detects CD reading error.
POSSIBLE CAUSE | • Defective CD (scratches or dirt) • CD changer (upper module) malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Play all the CDs in the changer. Are they read normally? | Yes | Go to Step 3.
No | Cannot read specific CDs. | Go to the next step.
Cannot read any CD. | Go to Step 3.
2 | Verify the condition of the CD when the error occurs. Is the CD normal? | Yes | Go to the next step.
No | Repair (remove foreign material, clean) or replace the CD, and go to the next step.
3 | Clear the DTC, and then insert a normal CD. Play the CD for 12 s or more. Is DTC 06: Er07 displayed? | Yes | Replace the CD changer (upper module).
No | DTC troubleshooting completed.