#
IGNITION COIL REMOVAL/INSTALLATION

BHE011801009W02

1. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)

2. Remove the battery cover.

3. Remove the negative battery cable. (See BATTERY REMOVAL/INSTALLATION.)

4. Remove the air cleaner duct. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

1 | Connector
2 | High-tension lead (See HIGH-TENSION LEAD REMOVAL/INSTALLATION.)
3 | Ignition coil

6. Install in the reverse order of removal.