#
DTC P0032

BHE010200001W03

DTC P0032 | Front HO2S heater control circuit high
--- | ---
DETECTION CONDITION | • The PCM monitors the front HO2S heater control voltage when the PCM turns the front HO2S heater on. If the control voltage is less than 25 % of the battery voltage, the PCM determines that the front HO2S heater control circuit voltage is high. Diagnostic support note • This is a continuous monitor (HO2S heater). • The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM. • PENDING CODE is available if the PCM detects the above malfunction condition during the first drive cycle. • FREEZE FRAME DATA is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Front HO2S heater malfunction • Connector or terminal malfunction • Open circuit in wiring harness between main relay terminal C and front HO2S terminal C • Short to GND in wiring harness between main relay terminal C and front HO2S terminal C • Open circuit in wiring harness between front HO2S terminal D and PCM terminal 1V • Short to GND in wiring harness between front HO2S terminal D and PCM terminal 1V • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT FRONT HO2S CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the front HO2S connector. • Inspect for poor connection (such as damaged/pulled-out pins, and corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
4 | INSPECT FRONT HO2S HEATER POWER CIRCUIT FOR OPEN CIRCUIT OR SHORT TO GND • Turn the ignition switch to the ON position (Engine off). • Measure the voltage between front HO2S terminal C (wiring harness-side) and body GND. • Is the voltage B+? | Yes | Go to the next step.
No | Repair or replace the wiring harness for a possible open circuit or short to GND, then go to Step 9.
5 | INSPECT FRONT HO2S HEATER CONTROL CIRCUIT FOR SHORT TO GND • Turn the ignition switch off. • Inspect for continuity between front HO2S terminal D (wiring harness-side) and body GND. • Is there continuity? | Yes | Repair or replace the wiring harness for a possible short to GND, then go to Step 9.
No | Go to the next step.
6 | INSPECT FRONT HO2S HEATER • Inspect the front HO2S heater. (See FRONT HEATED OXYGEN SENSOR (HO2S) INSPECTION.) • Is there any malfunction? | Yes | Replace the front HO2S, then go to Step 9. (See FRONT HEATED OXYGEN SENSOR (HO2S) REMOVAL/INSTALLATION.)
No | Go to the next step.
7 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, and corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
8 | INSPECT FRONT HO2S HEATER CONTROL CIRCUIT FOR OPEN CIRCUIT • Turn the ignition switch off. • Inspect for continuity between front HO2S terminal D (wiring harness-side) and PCM terminal 1V (wiring harness-side). • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for a possible open circuit, then go to the next step.
9 | VERIFY TROUBLESHOOTING OF DTC P0032 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Perform the DRIVE MODE 1 and 3. (See OBD DRIVE MODE.) • Is the PENDING CODE same as the DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION.)
No | Go to the next step.
10 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE.) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE.)
No | DTC troubleshooting completed.