#
FRONT FENDER PANEL REMOVAL/INSTALLATION

BHE091052110W01

1. Disconnect the negative battery cable.

2. Remove the front side turn lights. (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Remove the front combination lights. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

1 | Fastener
2 | Bolt A
3 | Bolt B
4 | Bolt C
5 | Bolt D
6 | Front fender panel

6. Install in the reverse order of removal.