#
SECONDARY SHUTTER VALVE (SSV) SOLENOID VALVE INSPECTION

BHE011301005W12

1. Disconnect the negative battery cable.

2. Remove the SSV solenoid valve. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)

3. Inspect for airflow using the steps in the table below.

  • If it is normal, inspect related wiring harnesses.
  • If there is any malfunction, replace the SSV solenoid valve.

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION.)

2. Inspect the following wiring harness for open or short (continuity check).

### Open circuit

  • If there is no continuity, the circuit is open. Repair or replace the harness.
  – SSV solenoid valve terminal B (harness-side) and PCM terminal 1L
  – SSV solenoid valve terminal A (harness-side) and main relay terminal C (harness-side)

### Short circuit

  • If there is continuity, the circuit is shorted. Repair or replace the harness.
  – SSV solenoid valve terminal B (harness-side) and body GND
  – SSV solenoid valve terminal A (harness-side) and power supply