#
REAR CROSSMEMBER CONSTRUCTION

BHE021428400T01

• Adoption of a six-point rubber-mounting system rear crossmember ensures link support stiffness and isolates vibration improving riding comfort and reducing road noise.

• Zero-stopper-clearance rubber bushings are installed at three points (the front, middle, and rear) of the crossmembers, six locations in total, so that they form a three-dimensional triangle.

• This construction provides the following benefits:

  – Suppresses rear crossmember turning when lateral forces are applied, ensuring high camber stiffness.
  – Bushing characteristics can be softened.
  – Suppresses vibrations transmitted to the vehicle body.

1 | Rear crossmember bushing
2 | Zero-stopper-clearance structure
3 | External force from tire