#
PID/DATA MONITOR TABLE

BHE080201046W07

PID name (definition) | Unit/Condition | Operation Condition (Reference) | Terminal
--- | --- | --- | ---
CCNT_RCM (Number of continuous DTCs) | — | • DTCs detected: 1-255 • No DTCs detected: 0 | —
D_ABAGR2 (Driver-side air bag module (inflator No.2) resistance) | Ohms | Under any condition: 1.5-3.7 ohms | 1G, 1J
D_CRSH_S (Driver-side side air bag sensor status) | OK/ COMM_FAIL/ INT_FAIL | • Sensor normal: OK • Sensor communication error: COMM_FAIL • Sensor internal circuit abnormal: INT_FAIL | 2Z, 2AA
DABAGR (Driver-side air bag module (inflator No.1) resistance) | Ohms | Under any condition: 1.5-3.7 ohms | 1S, 1V
D_PTENSFLT (Driver-side pre-tensioner seat belt circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES | 2P, 2S
DR_BUKL (Driver-side buckle switch status) | Buckled/ Unbuckled | • Driver-side buckle switch on: Buckled • Driver-side buckle switch off: Unbuckled | 2T
DR_CURTN (Driver-side curtain air bag module resistance) | Ohms | Under any condition: 1.4-3.2 ohms | 2V, 2Y
DR_PTENS (Driver-side pre-tensioner seat belt resistance) | Ohms | Under any condition: 1.5-3.1 ohms | 2P, 2S
DS_AB (Driver-side side air bag module resistance) | Ohms | Under any condition: 1.4-3.2 ohms | 2M, 2O
DS_AB_ST (Driver-side side air bag module circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 2M, 2O
DS_CURT_ST (Driver-side curtain air bag module circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 2V, 2Y
DS1_STAT (Driver-side air bag module (inflator No.1) circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 1S, 1V
DS2_STAT (Driver-side air bag module (inflator No.2) circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 1G, 1J
DSB_P_ST (Driver-side pre-tensioner seat belt circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES | 2P, 2S
FNT_CRSH_S (Crash zone sensor status) | OK/ COMM_FAIL/ INT_FAIL | • Sensor normal: OK • Sensor communication error: COMM_FAIL • Sensor internal circuit abnormal: INT_FAIL | 1B, 1C
OD_D_CRSH (Driver-side side air bag sensor status) | OK/ COMM_FAIL/ INT_FAIL | • Sensor normal: OK • Sensor communication error: COMM_FAIL • Sensor internal circuit abnormal: INT_FAIL | 2Z, 2AA
OD_D_CURT (Driver-side curtain air bag module circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 2V, 2Y
OD_DAB1_ST (Driver-side air bag module (inflator No.1) circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 1S, 1V
OD_DAB2_ST (Driver-side air bag module (inflator No.2) circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 1G, 1J
OD_DSAB_ST (Driver-side side air bag module circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 2M, 2O
OD_F_CRSH (Crash zone sensor status) | OK/ COMM_FAIL/ INT_FAIL | • Sensor normal: OK • Sensor communication error: COMM_FAIL • Sensor internal circuit abnormal: INT_FAIL | 1B, 1C
OD_P_CRSH (Passenger-side side air bag sensor status) | OK/ COMM_FAIL/ INT_FAIL | • Sensor normal: OK • Sensor communication error: COMM_FAIL • Sensor internal circuit abnormal: INT_FAIL | 2B, 2C
OD_P_CURT (Passenger-side curtain air bag module circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 2A, 2D
OD_PAB1_ST (Passenger-side air bag module (inflator No.1) circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 1M, 1P
OD_PAB2_ST (Passenger-side air bag module (inflator No.2) circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 1A, 1D
OD_PSAB_ST (Passenger-side side air bag module circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 2I, 2L
P_ABAGR2 (Passenger-side air bag module (inflator No.2) resistance) | Ohms | Under any condition: 1.4-2.9 ohms | 1A, 1D
P_PTENSFLT (Passenger-side pre-tensioner seat belt circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES | 2G, 2J
PABAGR (Passenger-side air bag module (inflator No.1) resistance) | Ohms | Under any condition: 1.4-2.9 ohms | 1M, 1P
P_CRSH_S (Passenger-side side air bag sensor status) | OK/ COMM_FAIL/ INT_FAIL | • Sensor normal: OK • Sensor communication error: COMM_FAIL • Sensor internal circuit abnormal: INT_FAIL | 2B, 2C
PS_AB (Passenger-side side air bag module resistance) | Ohms | Under any condition: 1.4-3.2 ohms | 2I, 2L
PS_AB_ST (Passenger-side side air bag sensor circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 2I, 2L
PS_CURTN (Passenger-side curtain air bag module resistance) | Ohms | Under any condition: 1.4-3.2 ohms | 2A, 2D
PS_CURT_ST (Passenger-side curtain air bag module circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 2A, 2D
PS_PTENS (Passenger-side pre-tensioner seat belt resistance) | Ohms | Under any condition: 1.5-3.1 ohms | 2G, 2J
PS1_STAT (Passenger-side air bag module (inflator No.1) circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 1M, 1P
PS2_STAT (Passenger-side air bag module (inflator No.2) circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Air bag module circuit resistance low: SQ_LOWRES | 1A, 1D
PSB_P_ST (Passenger-side pre-tensioner seat belt circuit status) | NORMAL/ OPEN/ SHRT_GND/ SHRT_B+/ SQ_LOWRES | • Related wiring harness normal: NORMAL • Related wiring harness circuit open: OPEN • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES | 2G, 2J
RCM_VOLT (IG1 voltage) | V | • Ignition switch is at ON: B+ • Other: 0 | 1W