#
VENTILATOR GRILLE REMOVAL/INSTALLATION

BHE091764810W01

## Driver's Side

1. Disconnect the negative battery cable.

2. Remove the instrument cluster.(See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)

3. Remove the dashboard garnish.(See DASHBOARD GARNISH REMOVAL/INSTALLATION.)

4. Pull the driver-side demister grille upward and detach clip A.

5. Pull the driver-side demister grille outward and remove it.

6. Install in the reverse order of removal.

## Passenger's Side

1. Disconnect the negative battery cable.

2. Remove the glove compartment.(See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

3. Remove the passenger-side air bag module.(See PASSENGER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

4. Pull the passenger-side demister grille upward and detach clip A.

5. Pull the passenger-side demister grille outward and remove it.

6. Install in the reverse order of removal.

## Center

1. Remove the ashtray panel. (See CONSOLE REMOVAL/INSTALLATION.)

2. Remove the center panel module installation screws and bolts, then pull the center panel module outward. (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)

3. Remove the screws.

4. Pull the ventilator grille outward and detach clips A and B.

5. Detach tab C and remove the ventilator grille.

6. Install in the reverse order of removal.