#
DRIVELINE/AXLE SPECIFICATIONS

BHE030001018T03

Item | Specification
--- | ---
Transmission type | MT | AT
Front axle
Bearing type | Angular ball bearing
Rear axle
Bearing type | Angular ball bearing
Rear drive shaft
Joint type | Wheel side | Bell joint
Differential side | Tripod joint
Shaft diameter | (mm {in}) | Left side: 31.0 {1.22} (Maximum diameter) 27.0 {1.06} (Minimum diameter) Right side: 34.0 {1.34} (Maximum diameter) 27.0 {1.06} (Minimum diameter) | Left side: 25.0 {0.98} Right side: 25.8 {1.02}
Rear differential
Reduction gear type | Hypoid gear
Differential gear type | Straight bevel gear
Ring gear size | (inch) | 8
Reduction ratio | 4.444 | 4.300
Number of gear teeth | Drive pinion | 9 | 10
Ring gear | 40 | 43
Differential oil | Type | Grade | API service GL-5
Viscosity | SAE 90
Capacity (approx. quantity) | (L {US qt, Imp qt}) | 1.3 {1.4, 1.1}
Propeller shaft
Length |  | (mm {in}) | L | 1,078 {42.44}
Diameter |  | (mm {in}) | D1 | 76 {3.0} | 82.6 {3.25}
D2 | 71.5 {2.81} | -
D3 | 76 {3.0} | -