#
PCM REMOVAL/INSTALLATION

BHE014018880W01

1. When replacing the PCM, perform the following:

  • PCM configuration (See PCM CONFIGURATION.)

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

4. When replacing the PCM on the vehicles with the immobilizer system, perform the following:

  • Immobilizer system component replacement/key addition and clearing (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING.)

5. Install in the reverse order of removal.

U.K. specs.

1 | PCM cover
2 | Set bolt (See Set Bolt Removal Note.) (See Set Bolt Installation Note.)
3 | PCM component

## Set Bolt Removal Note

1. Drill the set bolt using a drill bit with a diameter larger than the shank until the head is removed.

  • If the shank is remained, remove it using locking pliers.

2. Clean all foreign material from the PCM connectors.

## Set Bolt Installation Note

1. Install a new set bolt and tighten it until the neck of the bolt breaks off.

Except for U.K. specs.

1 | PCM cover
2 | PCM cooler
3 | PCM