#
WHEEL APRON PANEL COMPONENT INSTALLATION

BHE098053210B02

1. When installing new parts, position each part so that the section measurement aligns with the body dimension.

2. Drill holes for plug welds before installing new parts.

3. After temporarily installing new parts, make sure the related parts fit properly.

  Note

  • When replacing the wheel apron panel front and the wheel apron panel rear separately, weld 16 locations indicated by (A).

4. Plug the six weld location indicated by (B) when installing the apron reinforcement upper.