#
FRONT BELTLINE MOLDING REMOVAL/INSTALLATION

BHE091650641W01

1. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

2. Remove the power outer mirror installation screws and move the mirror to access the front end of the front beltline molding. (See POWER OUTER MIRROR REMOVAL/INSTALLATION.)

3. While partially peeling back the front beltline molding, detach tabs A along the direction (1) shown in the figure.

4. Remove clip B and front beltline molding.

5. Install in the reverse order of removal.