#
NEUTRAL SWITCH CONSTRUCTION/OPERATION (MT)

BHE014017640T02

• When the shift lever is in the neutral position, the contact closes (ON) and the PCM detects a voltage of 0 V. When the shift lever is not in the neutral position, the contact opens (OFF) and the PCM detects a voltage of 12 V.

1 | Neutral switch
2 | Push OFF (6MT)
3 | Push ON (5MT)
4 | Other then neutral (OFF)
5 | Neutral (ON)
6 | Neutral (ON)
7 | Except above
8 | PCM
9 | No load
10 | Load
11 | CPU