#
STEERING SYSTEM

BHE065001034W01

Item | Specifications
--- | ---
Steering wheel | Play | (mm {in}) | 0-30 {0-1.2}
Effort (reference value) | (N·m {kgf·cm, in·lbf}) | 5.0 {50, 44} or less
Steering shaft | Length | (mm {in}) | 508.5 {20.02}
Steering gear and linkage | Pinion shaft | Rotation torque | (N·m {kgf·cm, in·lbf}) | 1.2-2.0 {13-20, 11-17}
[Pull scale reading] | (N {kgf, lbf}) | 11.2-20.0 {1.15-2.03, 2.52-4.48}
Tie-rod end ball joint | Swinging torque | (N·m {kgf·cm, in·lbf}) | 0.6-2.0 {6-20, 5-17}
[Pull scale reading] | (N {kgf, lbf}) | 5.9-19.6 {0.61-1.99, 1.33-4.40}
Tie rod ball joint | Rotation torque | (N·m {kgf·cm, in·lbf}) | 0.68-2.45 {7.0-24.9, 6.1-21.6}
[Pull scale reading] | (N {kgf, lbf}) | 6.8-24.5 {0.70-2.49, 1.53-5.50}