#
AIR INTAKE ACTUATOR REMOVAL/INSTALLATION

BHE074061060W01

1. Disconnect the negative battery cable.

2. Remove the glove compartment. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

3. Remove the keyless unit. (See KEYLESS UNIT REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Air intake actuator connector
2 | Air intake actuator

5. Install in the reverse order of removal.