#
INTAKE MANIFOLD DISASSEMBLY/ASSEMBLY

BHE011301005W09

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | Bracket (13B-MSP (HIGH POWER))
2 | APV motor (13B-MSP (HIGH POWER))
3 | SSV switch
4 | VDI valve (See VDI Valve Assembly Note.)
5 | Gasket
6 | Blind cap
7 | Intake manifold

## VDI Valve Assembly Note

1. Apply grease to the VDI valve end as shown in the figure.