#
BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION

BHE091467001W01

1. To remove the bonnet latch, remove the seal plate. (See FRONT BUMPER REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

1 | Connector (Vehicle with theft-deterrent system)
2 | Bonnet latch
3 | Bonnet release lever (See Bonnet Release Lever Removal Note.)
4 | Bonnet release cable

3. Install in the reverse order of removal.

4. Adjust the bonnet. (See BONNET ADJUSTMENT.)

## Bonnet Release Lever Removal Note

1. Pull the lever.

2. While pushing the tab in the direction of the arrow using a tape-wrapped, small flathead screwdriver, detach it from the dashboard.

  Caution

  • Remove the bonnet release lever while taking care not to damage the bonnet release cable with the flathead screwdriver.

3. Under the condition in Step 2, pull the bonnet release lever outward, then remove it from the dashboard.