#
REAR COMBINATION LIGHT REMOVAL/INSTALLATION

BHE091851150W01

1. Disconnect the negative battery cable.

2. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

3. Remove the trunk side trim. (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Nut
2 | Connector
3 | Rear combination light
4 | Socket
5 | Rear turn light bulb
6 | Back-up light bulb
7 | Stop/taillight bulb

5. Install in the reverse order of removal.