#
SEQUENTIAL DYNAMIC AIR INTAKE SYSTEM (S-DAIS) CONTROL BLOCK DIAGRAM

BHE014000140T16

• The PCM determines the engine conditions based on each input signal and sends signals to the SSV solenoid valve, the APV motor (13B-MSP (High Power)), the VDI solenoid valve, and the VFAD solenoid valve (13B-MSP (High Power)).

1 | ECT sensor
2 | TP sensor
3 | MAF sensor
4 | Eccentric shaft position sensor
5 | BARO sensor
6 | PCM
7 | SSV solenoid valve
8 | APV motor (13B-MSP (High power))
9 | VDI solenoid valve
10 | VFAD solenoid valve (13B-MSP (High power))