#
DTC B2434, B2435, B2691

BHE080201046W22

DTC | B2434 | Driver-side front buckle switch circuit short to body ground
--- | --- | ---
B2435 | Driver-side front buckle switch circuit resistance not within specification
B2691 | Driver-side front buckle switch circuit open or short to power supply
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only the detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • Malfunction in the driver-side front buckle switch circuit
POSSIBLE CAUSE | • Malfunction of the connectors between the driver-side front buckle switch and SAS unit • Open or short circuit in the wiring harness between the driver-side front buckle switch and SAS unit • Driver-side front buckle switch malfunction • SAS unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT DRIVER-SIDE BUCKLE SWITCH CIRCUIT • Using the WDS or equivalent, verify the following PID/DATA monitor. (See PID/DATA MONITOR TABLE.) – DR_BUKL • Is the driver-side front buckle switch normal? | Yes | [Present malfunction diagnosis] • Replace the SAS unit. (See SAS UNIT REMOVAL/INSTALLATION.) [Past malfunction diagnosis] • DTC troubleshooting completed.
No | Go to the next step.
2 | INSPECT DRIVER-SIDE BUCKLE MODULE • Turn the ignition switch to the LOCK position. • Disconnect the negative battery cable and wait for 1 min or more. • Remove the driver-side front buckle. (See FRONT BUCKLE REMOVAL/INSTALLATION.) • Inspect the driver-side front buckle switch. (See FRONT BUCKLE SWITCH INSPECTION.) • Is the driver-side front buckle switch normal? | Yes | Go to the next step.
No | Replace the driver-side front buckle. (See FRONT BUCKLE REMOVAL/INSTALLATION.)
3 | INSPECT WIRING HARNESS BETWEEN DRIVER-SIDE BUCKLE SWITCH AND GROUND • Inspect the wiring harness between driver-side front buckle switch terminal H (manual seat) or terminal C (power seat) and ground for the following: – Short to power supply – Open circuit • Is the wiring harness normal? | Yes | Go to the next step.
No | Replace the wiring harness.
4 | INSPECT WIRING HARNESS BETWEEN DRIVER-SIDE BUCKLE SWITCH AND SAS UNIT Warning • Handling the air bag system components improperly can accidentally deploy the air bag modules and pre-tensioner seat belts, which may seriously injure you. Read the service warnings and cautions before handling the air bag system components. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.) • Turn the ignition switch to the LOCK position. • Disconnect the negative battery cable and wait for 1 min or more. • Remove the column cover. • Disconnect the clock spring connector. • Remove the glove compartment. • Disconnect the passenger-side air bag module connector. • Disconnect the driver and passenger-side side air bag module connectors. • Disconnect the driver and passenger-side curtain air bag module connectors. • Remove the rear door lower trim. • Disconnect the driver and passenger-side pre-tensioner seat belt connectors. • Partially peel back the floor covering. • Disconnect the SAS unit connector. • Inspect the wiring harness between SAS unit terminal 2T and driver-side front buckle switch terminal G (manual seat) or terminal D (power seat) for the following: – Short to ground – Short to power supply – Open circuit • Is the wiring harness normal? | Yes | [Present malfunction diagnosis] • Replace the SAS unit. (See SAS UNIT REMOVAL/INSTALLATION.) [Past malfunction diagnosis] • DTC troubleshooting completed.
No | Replace the wiring harness.