#
NOISE FILTER REMOVAL/INSTALLATION

BHE092066869W01

## Brake Light Noise Filter

1. Disconnect the negative battery cable.

2. Remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

3. Peel off the tape.

4. Disconnect the connector and remove the brake light noise filter.

5. Install in the reverse order of removal.

## Rear Window Defroster Noise Filter

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (2) Console (See CONSOLE REMOVAL/INSTALLATION.)
  (3) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (4) Rear pillar trim (See REAR PILLAR TRIM REMOVAL/INSTALLATION.)
  (5) Rear package center trim, rear package side trim (See REAR PACKAGE TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Bolt
2 | Connector
3 | Noise filter

4. Install in the reverse order of removal.