#
SUNROOF UNIT DISASSEMBLY/ASSEMBLY

BHE091569850W03

1. Remove the glass panel. (See GLASS PANEL REMOVAL/INSTALLATION.)

2. Disassemble in the order indicated in the table.

3. Assemble in the reverse order of disassembly.

1 | Drip rail
2 | Drip guide
3 | Rear stopper
4 | Sunshade
5 | Sunroof motor (See Sunroof Motor Assembly Note.)
6 | Set plate
7 | Guide
8 | Decoration link
9 | Drive unit
10 | Frame

## Sunroof Motor Assembly Note

  Note

  • If the guide is removed, initial position setting of the sunroof motor will be required. After installing the sunroof unit, perform initial position setting using the following procedure.

1. Press the CLOSE switch to fully close the glass panel.

2. When the glass panel reaches the fully closed position, temporarily release the CLOSE switch and press it again for approx. 13 s continuously. Continue pressing the switch until the glass panel automatically stops at the fully closed position after reaching the mechanical lock position.

3. When the glass panel stops at the fully closed position, temporarily release the CLOSE switch, then press it again within 5 s and hold.

  Note

  • Press the CLOSE switch continuously until the glass panel opens to the fully open position, returns to the fully closed position and then stops.

4. Release the CLOSE switch when the glass panel stops at the fully closed position.