#
REAR DOOR LOWER TRIM REMOVAL/INSTALLATION

BHE091768400W01

1. Remove the grip cover, then remove screws A.

2. Using a small flathead screwdriver, open the cap and remove screw B.

3. Remove the cover while rotating it to the front.

4. Detach clips A, B, locator pins C, and tabs D from the rear door using a fastener remover.

5. Remove the rear door lower trim.

6. Install in the reverse order of removal.