#
FUEL PUMP RESISTOR INSPECTION

BHE011413350W04

## Resistance Inspection

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION.)

2. Remove the fuel pump resister. (See FUEL PUMP RESISTOR REMOVAL/INSTALLATION.)

3. Verify that the continuity between the fuel pump resister terminal A and B is within the specification.

  • If not within the specification, replace the fuel resistor.

  Fuel pump resistor continuity
  0.304-0.336 ohms (20 °C {68 °F})